|  |  |  |  |
| --- | --- | --- | --- |
| Line | R12 | R13 | Purpose |
| 66 | 0x01 | 0xE7 | Sets Data for drawing the line |
| 276 | 0x00 | 0xB0 or’d with row # | Specifies row |
| 288 | 0x00 | 0x10 or’d with row # | Specifies row |
| 294 | 0x00 | 0x00 or’d with row # | Specifies row |

|  |  |  |
| --- | --- | --- |
| Line | Command/Data | 8-bit packet |
| 66 | Data | 11100111 |
| 276 | Command | 0xB1 |
| 288 | Command | 0x10 |
| 294 | Command | 0x01 |